
# Creality 3D K1 machine uses cura slicing software.

### 1. Download Slicing Software

Need to download cura5 slicing software and install it yourself:

Download link: [GitHub - Ultimaker/Cura: 3D printer / slicing GUI built on top of the Uranium framework](https://github.com/Ultimaker/Cura)




### 2. Add printer


1. Entrance




2. Select K1 similar machine :Ender-3 S1



3. Renamed to Creality K1 or other name。



4. Just configure it to the K1 machine size, don't forget to start and end gcode synchronously。



Start G-code**(To keep newlines):**

M140 S0

M104 S0


START\_PRINT EXTRUDER\_TEMP=220 BED\_TEMP=55

End G-code**(To keep newlines):**


END\_PRINT

### 3. Import gcode configuration file.


1. In the operation drop-down box on the right sidebar, click Manage Configuration Files:




2. Click the import button to upload the configuration file of the K1 machine we prepared in advance (tutorial attachment):



After the import is successful, we find the configuration file, select it, and click the fold button on the right:



3. Finally click to activate the configuration file to take effect:




K1 series machine configuration file:

[cura\_k1\_pla.curaprofile](https://drive.weixin.qq.com/s?k=AGMAvQfiAAgIpY25weAG0AVAaLAEk)

### 4. Save to desktop after slicing

After all configuration operations are completed, we import the model, select the imported configuration file, and click the slice button:



1. After slicing is successful, we save the gcode file to the desktop/disk space。

descript

© 2014-2023 Shenzhen Chuangxiang 3D Technology Co., Ltd. All rights reserved.

Feedback email: kefu@creality.com